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Stationary Concrete Mixing Plant
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Fasting Moving Concrete Mixing Plant
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Mobile Concrete Mixing Plant
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Simple Mobile Concrete Mixing Plant
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HiSnumber (1% & &FDevice Name| B Smode! RHallocation
WHBAHBEL PLB00-1, JS500, SENFIR}, 7K PLBOO-1, JS500, preumatic unloading,
LT20160065|  Simple mobile JYHZS25 |, MARRA M, KFHEE|  cunulative measurement of cement and fly
mixing plant #, MHEH ash, water time control, simple control
BHBIREHEE PL1200-2, JS750, SENEDRY, 7k|  PL1200-2, JS7S0, pneumatic unloading,
L120160090| ~ Simple mobile JYHZS35 |JR. MRARIIR, KEHERE|  cumulative measurement of cement and fly
mixing plant #l, WHEH ash, water time control, simple control
WHBERE PL1600-3, JS1000, 3. 83K PL1600-3, JS1000, 3.8 meter discharge,
L120160170|  Simple mobile JYHZSS0 |#, FENEH, kiR MR | manual discharge, cumulative measurement of
mixing plant it KEEEH, HHEH)|  cement and fly ash, water time control,
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FSmodel WZS% 5% S50 IS5 HZ590 HZS120 IS8
7 Theorelcal produciviy 2m'n B som' . T5m . Som'm, 2om' . 8o’/
hEn B8 nodel J8500 45750 451000 1500 451500 452000 453000
Mong host EAIEDrive power 18.5kw 30kw 218.5kw 2x30kw 230w 27w 2650
BEBEMaxinun parice szs|___eomm Bomm Bomm Bonm Bomm omm o
Bhagoregale T0-18004g ] =2% | (0-2500kg | =24 (0-2500kg | =25 (0-3600kp) 2% 0-3000kg) 2% | x2500kg ) 2% | (0-3500kq ] =2%
BREE Kifcement (03004 ) = 1% | (0-300kg) =1%| (0-5004g) =1% | (0-7ODkg) = 1%| (0-700kq) = 1% | (0-T100kg] = 15| (0-1600Kg) =1%)
Weghing BRAFY ash (0-2504g) +1% | (0-400kg) = 1% | (0-400kq) = 1% | (0-500kg) = 1% | (0-600kg) =1%
Range Kuater T0-1506g) + 1% | (0-2004g) =1%| (0-3004g) +1% | (0-300kg) =1%| (0-500kg) 1% | (0-500kg) =1% | (0-800kg) =1%
A fiadmixure 10-30kg) =1% | (0-30kg) =1% | (0-40kg) =1% | (0-40kg) £1% | (0-60kp) =1% | (0-B0kg) 1% | (0-80kg) =%
iR EDischarge height 3800mm 3800mm 3800mm 3800mm 4000 200mm 200mm
SHUHEWhoe machine poner B S5k T 110w 110w 1450 190w
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i ammmsmntlsanu s atusmalsabnmpdinnsannmtedbdubbetbilindu.ozipm o il

HE model KHZS35 KHZS50 KHZS75 KHZS100
BipER
Theoretical productivity - = e b
BEHEHN Mixing host JS1250/750 | JS1500/1000 | JS2250/1500 | JS3000/2000
BFLRS Batching system PLD1200 PLD1600 PLD2400 PLD3200
SDRERE  Discharge height 3.8 3.8M 3.8M 3.8M
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HE  model YHZS35 YHZS50 YHZS75 YHZS100
Theoratﬁi%ipzictivity i i i e
HFEEH Mixing host JS1250/750 | JS1500/1000 | JS2250/1500 | JS3000/2000
BMARS Batching system PLD1200 PLD1600 PLD2400 PLD3200
EVNE Discharge height 3.8M 3.8M 3.8M 3.8M





